**Cisco Packet Tracer**

**Network Configuration Documentation**

**Kurt Robin P. Colonia**

**Scenario: Company Network**

* Main Office w/ 3 subnets
* Branch Office with 2 subnets
* ISP Router with DNS + 5 websites simulating the Internet.

Addressing Plan:

* Main Office LANs:
  + HR: 10.0.1.0/24
  + IT: 10.0.2.0/24
  + Finance: 10.0.3.0/24
* Branch LANs:
  + Sales: 10.1.1.0/24
  + Support: 10.1.2.0/24
* WAN Links:
  + Main -> Branch: 192.168.10.0/30
  + Main -> ISP: 192.168.20.0/30
* ISP (Public Network):
  + DNS Server: 203.0.113.10
  + Websites: 203.0.113.20 - 203.0.113.24riot